**Add two 8-bit numbers with carry**

LXI H,3000H;

MOV A,M;

INX H;

MOV B,M;

MVI C,00H;

ADD B;

JNC X;

INR C;

X: INX H;

MOV M,A;

INX H;

MOV M,C;

hlt